Manual Update Instructions:

1. Power on your Sub Phatty
2. Push both PITCH AMT and HARD SYNC, and while holding, push ACTIVATE PANEL twice
3. Load C6
4. Set Midi ports to Sub Phatty
5. Drag the included syx file into C6, and mark it
6. Click on Send
